Figure 2: Screen shot of test tube system